A B C D G M O P R S T Z

## A

APIM_APPLICATION_TOKEN_VALIDITY_PERIOD - Static variable in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.constants.RaspberrypiConstants
APIUtil - Class in org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util
  This class provides utility functions used by REST-API.
APIUtil() - Constructor for class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.APIUtil

## B

BULB_CONTEXT - Static variable in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.constants.RaspberrypiConstants

## C

contextDestroyed(ServletContextEvent) - Method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.listener.RaspberryPIPermissionUpdateListener
contextInitialized(ServletContextEvent) - Method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.listener.RaspberryPIPermissionUpdateListener
createSensorData(List<Record>) - Static method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.APIUtil
  Creates the SensorDatas from records.
createSensorData(Record) - Static method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.APIUtil
  Create a SensorRecord object out of a Record object
createZipFile(String, String, String, String, String, String, String) - Method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.ZipUtil

## D

DEVICE_TYPE - Static variable in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.constants.RaspberrypiConstants
downloadSketch(String, String) - Method in interface org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.RaspberryPiService
  download the agent.
downloadSketch(String, String) - Method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.RaspberryPiServiceImpl

## G

getAllEventsForDevice(String, String, List<SortByField>) - Static method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.APIUtil
getAnalyticsDataAPI() - Static method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.APIUtil
getAPIManagementProviderService() - Static method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.APIUtil
getAuthenticatedUser() - Static method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.APIUtil
getAuthorizationManager() - Static method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.listener.RaspberryPIPermissionUpdateListener
getContent() - Method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.ZipUtil.TemplateFile
getDeviceAccessAuthorizationService() - Static method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.APIUtil
getDeviceManagementService() - Static method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.APIUtil
getFileName() - Method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.ZipArchive
getFileName() - Method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.ZipUtil.TemplateFile
getId() - Method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.dto.SensorRecord
  Gets the id.
getJWTClientManagerService() - Static method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.APIUtil
getRaspberryPiTemperatureStats(String, long, long) - Method in interface org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.RaspberryPiService
  Retreive Sensor data for the device type
getRaspberryPiTemperatureStats(String, long, long) - Method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.RaspberryPiServiceImpl
getSortedSensorData(Map<String, SensorRecord>, List<SearchResultEntry>) - Static method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.APIUtil
getTenantConfigurationManagementService() - Static method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.APIUtil
getTenantDomainOftheUser() - Static method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.APIUtil
getUserStoreManager() - Static method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.listener.RaspberryPIPermissionUpdateListener
getValues() - Method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.dto.SensorRecord
  Gets the values.
getZipFileContent() - Method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.ZipArchive

## M

MQTT_ADAPTER_TOPIC_PROPERTY_NAME - Static variable in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.constants.RaspberrypiConstants

## O

org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl - package org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl
org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.constants - package org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.constants
org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.dto - package org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.dto
org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.exception - package org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.exception
org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.listener - package org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.listener
org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util - package org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util

## P

PERM_ENROLL_RASPBERRYPI - Static variable in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.constants.RaspberrypiConstants
PERM_OWNING_DEVICE_VIEW - Static variable in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.constants.RaspberrypiConstants

## R

RaspberrypiConstants - Class in org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.constants
RaspberrypiConstants() - Constructor for class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.constants.RaspberrypiConstants
RaspberrypiException - Exception in org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.exception
RaspberrypiException(String) - Constructor for exception org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.exception.RaspberrypiException
RaspberrypiException(String, Throwable) - Constructor for exception org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.exception.RaspberrypiException
RaspberryPIPermissionUpdateListener - Class in org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.listener
RaspberryPIPermissionUpdateListener() - Constructor for class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.listener.RaspberryPIPermissionUpdateListener
RaspberryPiService - Interface in org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl
RaspberryPiServiceImpl - Class in org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl
RaspberryPiServiceImpl() - Constructor for class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.RaspberryPiServiceImpl
ROLE_NAME - Static variable in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.constants.RaspberrypiConstants

## S

SCOPE - Static variable in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.constants.RaspberrypiConstants
SensorRecord - Class in org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.dto
SensorRecord() - Constructor for class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.dto.SensorRecord
setContent(String) - Method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.ZipUtil.TemplateFile
setFileName(String) - Method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.ZipUtil.TemplateFile
setId(String) - Method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.dto.SensorRecord
  Sets the id.
setValues(Map<String, Object>) - Method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.dto.SensorRecord
  Sets the values.
STATE_OFF - Static variable in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.constants.RaspberrypiConstants
STATE_ON - Static variable in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.constants.RaspberrypiConstants
switchBulb(String, String) - Method in interface org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.RaspberryPiService
switchBulb(String, String) - Method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.RaspberryPiServiceImpl

## T

TEMPERATURE_EVENT_TABLE - Static variable in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.constants.RaspberrypiConstants
toString() - Method in class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.dto.SensorRecord

## Z

ZipArchive - Class in org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util
  This is an utility class to hold zip files.
ZipArchive(String, byte[]) - Constructor for class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.ZipArchive
ZipUtil - Class in org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util
  This is used to create a zip file that includes the necessary configuration required for the agent.
ZipUtil() - Constructor for class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.ZipUtil
ZipUtil.TemplateFile - Class in org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util
ZipUtil.TemplateFile() - Constructor for class org.wso2.carbon.device.mgt.iot.raspberrypi.service.impl.util.ZipUtil.TemplateFile

A B C D G M O P R S T Z

Copyright © 2017 WSO2. All rights reserved.